This is the Virtual COM Driver from Silicon Labs, required by RF Explorer

Version: 6.7.5 (All Windows versions newer than WinXP)
Version: 6.7 (WinXP)

Supported OS versions: Windows 10 (64/32) 8.1 (64/32), 7 (64/32), Vista (64/32), Windows Server, and Windows XP

Installation instructions:
* Disconnect RF Explorer and close all applications
* Go to control panel and uninstall any existing "Silicon Laboratories CP210x..." entry you may find.
* Reboot your PC
* Use the CP210x_Drivers_WindowsXP.zip file for Windows XP
* Use the CP210x_Drivers_Windows-7-8-10.zip file for Windows 10, 8.1, 7, Vista
* Inside the driver zip file there are two options based on your specific hardware:
    * For 32 bits systems, run the included file CP210x_VCP_Windows\CP210xVCPInstaller_x86.exe.
    * For 64 bits systems, run the included file CP210x_VCP_Windows\CP210xVCPInstaller_x64.exe.
* Reboot your PC
* Connect RF Explorer device and run RF Explorer for Windows

---